{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["Sheet1","Sheet2"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":73,"n_cols":6,"rows_kept":73,"cut":false,"hidden":false,"merged":[[0,5,0,6],[1,5,1,6],[2,5,2,6],[3,5,3,6],[4,5,4,6],[5,5,5,6],[6,5,6,6],[7,5,7,6],[8,5,8,6],[9,5,9,6],[10,5,10,6],[11,5,11,6],[12,5,12,6],[13,5,13,6],[14,5,14,6],[15,5,15,6],[16,5,16,6],[17,5,17,6],[18,5,18,6],[19,5,19,6],[20,5,20,6],[21,5,21,6],[22,5,22,6],[23,5,23,6],[24,5,24,6],[25,5,25,6],[26,5,26,6],[27,5,27,6],[28,5,28,6],[29,5,29,6],[30,5,30,6],[31,5,31,6],[32,5,32,6],[33,5,33,6],[34,5,34,6],[35,5,35,6],[36,5,36,6],[37,5,37,6],[38,5,38,6],[39,5,39,6],[40,5,40,6],[41,5,41,6],[42,5,42,6],[43,5,43,6],[44,5,44,6],[45,5,45,6],[46,5,46,6],[47,5,47,6],[48,5,48,6],[49,5,49,6],[50,5,50,6],[51,5,51,6],[52,5,52,6],[53,5,53,6],[54,5,54,6],[55,5,55,6],[56,5,56,6],[57,5,57,6],[58,5,58,6],[59,5,59,6],[60,5,60,6],[61,5,61,6],[62,5,62,6],[63,5,63,6],[64,5,64,6],[65,5,65,6],[66,5,66,6],[67,5,67,6],[68,5,68,6],[69,5,69,6],[70,5,70,6],[71,5,71,6],[72,5,72,6]]}
["十进制","Modbus位地址","说明","数据类型","操作性","上限"]
[{"$f":"HEX2DEC(B2)","v":0},0,"起动仪器","布尔型","可读写"]
[1,1,"复位仪器","布尔型","可读写"]
[2,2,"仪器当前运行状态","布尔型","可读写"]
[3,3,"上位机参数写入确认","布尔型","可读写"]
[4,4,"蜂鸣器","布尔型","可读写"]
[5,5,"压力校准","布尔型","可读写"]
[6,6,"压差校准","布尔型","可读写"]
[7,7,"升级（rtu有 tcp没有）","布尔型","可读写"]
[0]
["十进制","Modbus字地址","说明",null,"操作性"]
[{"$f":"HEX2DEC(B12)","v":1000},"3E8","参数编号","字符串","可读写"]
[1001,"3E9","当前参数名称","字符串","可读写"]
[1002,"3EA","当前参数名称","字符串","可读写"]
[1003,"3EB","当前参数名称","字符串","可读写"]
[1004,"3EC","当前参数名称","字符串","可读写"]
[1005,"3ED","当前参数名称","字符串","可读写"]
[1006,"3EE","充气时间","整型","可读写","0-30000ms"]
[1007,"3EF","平衡时间","整型","可读写","0-30000ms"]
[1008,"3F0","检测时间","整型","可读写","0-30000ms"]
[1009,"3F1","排气时间","整型","可读写","0-30000ms"]
[1010,"3F2","解除输出2时间","整型","可读写"]
[1011,"3F3","延时1","整型","可读写"]
[1012,"3F4","延时2","整型","可读写"]
[1013,"3F5","充气压力上限低位","浮点型","可读写"]
[1014,"3F6","充气压力上限高位","浮点型","可读写"]
[1015,"3F7","充气压力下限低位","整型","只可读"]
[1016,"3F8","充气压力下限高位","整型","只可读"]
[1017,"3F9","平衡压差上限低位","整型","可读写"]
[1018,"3FA","平衡压差上限高位","整型","可读写"]
[1019,"3FB","平衡压差下限低位","浮点型","可读写"]
[1020,"3FC","平衡压差下限高位","浮点型","可读写"]
[1021,"3FD","允许泄漏量上限低位",null,"只可读"]
[1022,"3FE","允许泄漏量上限高位",null,"只可读"]
[1023,"3FF","允许泄漏量下限低位","浮点型","只可读"]
[1024,400,"允许泄漏量下限高位","浮点型","只可读"]
[1025,401,"等效容积低位","浮点型","只可读"]
[1026,402,"等效容积高位","浮点型","只可读"]
[1027,403,"压力单位","浮点型","可读写"]
[1028,404,"泄漏量单位","浮点型","可读写"]
[1034,"40A","仪器状态","字符串","只可读"]
[1035,"40B","大漏泄漏量低位（平衡压差）","浮点型","只可读"]
[1036,"40C","大漏泄漏量高位（平衡压差）","浮点型","只可读"]
[1037,"40D","大漏泄漏量单位（压差单位）","字符串","只可读"]
[1038,"40E","微漏泄漏量低位（泄漏量）","字符串","只可读"]
[1039,"40F","微漏泄漏量高位（泄漏量）","字符串","只可读"]
[1040,410,"微漏泄漏量单位（泄漏量）","字符串","只可读"]
[1041,411,"测试结果","字符串","只可读"]
[1048,418,"后台压力低位","整型","只可读"]
[1049,419,"后台压力高位","整型","只可读"]
[1050,"41A","后台压差低位","整型","只可读"]
[1051,"41B","后台压差高位","整型","只可读"]
[1057,421,"记录-测试压力低位","整型","只可读"]
[1058,422,"记录-测试压力高位","整型","只可读"]
[1059,423,"记录-压力单位","整型","只可读"]
[1060,424,"记录-压力单位","整型","只可读"]
[1061,425,"记录-压力单位","整型","只可读"]
[1062,426,"记录-测试泄漏量低位"]
[1063,427,"记录-测试泄漏量高位"]
[1064,428,"记录-泄漏量单位"]
[1065,429,"记录-泄漏量单位"]
[1066,"42A","记录-泄漏量单位"]
[1067,"42B","记录-泄漏量单位"]
[1076,434,"modbus从机号"]
[1077,435,"IP第一段地址"]
[1078,436,"IP第二段地址"]
[1079,437,"IP网关第一段地址"]
[1080,438,"IP网关第二段地址"]
[1081,439,"子网掩码地址1默认255"]
[1082,"43A","子网掩码地址2默认255"]
[1083,"43B","固定IP启用开关（写值就为启动，0关闭）"]
[1086,"43E","压差差值低位"]
[1087,"43F","压差差值高位"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}